|  |  |
| --- | --- |
| **卡波姆树脂Carbomero 940** | |
| **参数 Param** | **数值 Value** |
| 沸点Boiling Point | 116 °C |
| 密度 Density | 1.2 g/mL at 25 °C |
| 折射率 Refractive Index | *n*20/D 1.442 |
| 闪点 Flash point | 100 °C |
| 储存条件 Storage Condition | 2-8°C |
| 溶解度Solubility | Swellable in water and glycerin and, after neutralization,in ethanol (95%). Carbomers do not dissolve but merelyswell to a remarkable extent, since they are three-dimensionallycrosslinked microgels. |
| 形态 Form | Powder |
| 颜色 Color | White |
| 水溶解性 Solubleness | Soluble in water. |
| InChIKey | WLAMNBDJUVNPJU-UHFFFAOYSA-N |
| EPA化学物质信息 Chemical Substances information | 2-Propenoic acid, homopolymer(9003-01-4) |

安全说明 Safety Description

|  |  |
| --- | --- |
| **卡波姆树脂 Carbomer** | |
| **参数 Parameter** | **数值 Value** |
| 危险品标志 Dangerous mark | C,T,Xi |
| 危险类别码 Class of risk | 45-46-34-36/37/38 |
| 安全说明 Safety description | 53-45-36-27-26 |
| 危险品运输编号 Dangerous Goods transportation number | UN 3265 8/PG 3 |
| WGK Germany | 3 |
| RTECS号 | AT4680000 |
| TSCA | Yes |
| 海关编码  HS CODE | 39069090 |